**F-1 MW Checklist for Physics 103**

On each table, check the presence of

1 stand to suspend the spheres

1 double-beam balance

1 graduated plastic beaker

In the lab room, check the presence of

At least 4 sets of assorted spheres of aluminum, lead, wood and magnesium.

Slotted weights

On each table, check for functionality

The double-beam balance does not have a zero error. If it does, check that it can be adjusted using the screw on the right of the balance.

The plastic beaker does not have any crack to allow water to leak from it.

The plastic beaker is graduated and the markings are legible.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |