**M-5 Checklist**

On each table, check the presence of:

1 spring gun

1 brass ball

1 protractor

1 catcher with a rubber band attached to one end

A platform and stand to hold the entire assembly

1 plum bob string suspended from the protractor

1 wooden catcher

In the lab room, check the presence of:

Plumb bobs

Extra rubber bands

 Rulers

White paper

On each table, check for functionality:

The angle and level of the platform can be adjusted

The angle markings on the protractor are intact and legible

The ball fits securely in the spring gun

The spring gun loads and fires appropriately

The height of the length holding the catcher can be adjusted

The protractor remains fairly stable and does not wobble

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |