**E-3 Checklist**

On each table, check the presence of:

A plugboard (breadboard)

2 multimeters and 2 pairs of multimeter probes.

1 DC Power supply

Resistances of 1kΩ, 2.2kΩ and 4.7Ω

Metal connectors

In the lab room, check the presence of:

Power cables

Banana cables

On each table, check for functionality:

The power supply can turn on and can be adjusted to 15V

The resistors are not internally shorted.

The resistors fit tightly into the slots of the breadboard

The metal connectors fit tightly into the slots of the breadboard and at least 2 of these are shorted internally.

The vertical slots at the two sides of the breadboard are all shorted.

The multimeters switch on and function satisfactorily.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| -- | -- | -- | -- | -- | -- | -- | -- | -- |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| -- | -- | -- | -- | -- | -- | -- | -- | -- |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |